# Attack

Selected AP:

Selected Clients:

deauth selected:
sends deauthentication frames and dissociation frames to the selected client(s) in the selected WiFi network.
deauth all:
sends deauthentication frames and dissociation frames as broadcast to all clients in the selected WiFi network.
beacon spam:
sends beacon frames with the same SSID as the selected WiFi access point.
random beacon spam:
sends beacon frames with a random SSID .