<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="74.93" y1="73.66" x2="43.18" y2="73.66" width="0.762" layer="20"/>
<wire x1="43.18" y1="12.7" x2="74.93" y2="12.7" width="0.762" layer="20"/>
<wire x1="43.18" y1="73.66" x2="43.18" y2="12.7" width="0.762" layer="20"/>
<wire x1="74.93" y1="12.7" x2="74.93" y2="73.66" width="0.762" layer="20"/>
<hole x="53.34" y="69.85" drill="0.4"/>
<hole x="68.58" y="52.07" drill="0.4"/>
<hole x="68.58" y="33.02" drill="0.4"/>
<hole x="53.34" y="16.51" drill="0.4"/>
</plain>
<libraries>
<library name="Capacitor">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPRD550W60D1025H1250B">
<description>Radial Non-Polarized Capacitor, 5.50 mm pitch, 10.25 mm body diameter, 12.50 mm body height
&lt;p&gt;Radial Non-Polarized Capacitor package with 5.50 mm pitch (lead spacing), 0.60 mm lead diameter, 10.25 mm body diameter and 12.50 mm body height&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Synthesizer Components">
<packages>
<package name="AS3360-FOOTPRINT">
</package>
<package name="PAD-FOOTPRINT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Capacitor" package="CAPRD550W60D1025H1250B" value="4.7nF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="U$4" library="Synthesizer Components" package="AS3360-FOOTPRINT" value="AS3360">
</element>
<element name="U$12" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$13" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$14" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$15" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$16" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$20" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$33" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$40" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$42" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="C2" library="Capacitor" package="CAPRD550W60D1025H1250B" value="4.7nF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="U$1" library="Synthesizer Components" package="AS3360-FOOTPRINT" value="AS3360">
</element>
<element name="U$2" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$3" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$5" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$6" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$7" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$8" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$9" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$10" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$11" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="C3" library="Capacitor" package="CAPRD550W60D1025H1250B" value="4.7nF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="U$17" library="Synthesizer Components" package="AS3360-FOOTPRINT" value="AS3360">
</element>
<element name="U$18" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$19" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$21" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$22" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$23" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$24" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$25" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$26" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
<element name="U$27" library="Synthesizer Components" package="PAD-FOOTPRINT" value="PAD">
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$4" pad="GND"/>
<contactref element="C1" pad="1"/>
<contactref element="U$16" pad="PAD"/>
</signal>
<signal name="N$1">
<contactref element="U$4" pad="VE1"/>
<contactref element="U$4" pad="VO1"/>
</signal>
<signal name="N$2">
<contactref element="U$4" pad="VE2"/>
<contactref element="U$4" pad="VO2"/>
</signal>
<signal name="N$6">
<contactref element="U$4" pad="VC1"/>
<contactref element="U$40" pad="PAD"/>
</signal>
<signal name="N$12">
<contactref element="U$4" pad="II1"/>
<contactref element="U$33" pad="PAD"/>
</signal>
<signal name="N$14">
<contactref element="U$4" pad="IO1"/>
<contactref element="U$42" pad="PAD"/>
</signal>
<signal name="N$20">
<contactref element="U$4" pad="VC2"/>
<contactref element="U$13" pad="PAD"/>
</signal>
<signal name="N$23">
<contactref element="U$4" pad="II2"/>
<contactref element="U$12" pad="PAD"/>
</signal>
<signal name="N$25">
<contactref element="U$4" pad="OI2"/>
<contactref element="U$14" pad="PAD"/>
</signal>
<signal name="S$10">
<contactref element="U$4" pad="EE"/>
<contactref element="U$20" pad="PAD"/>
</signal>
<signal name="S$13">
<contactref element="U$15" pad="PAD"/>
<contactref element="U$4" pad="CC"/>
</signal>
<signal name="N$3">
<contactref element="U$4" pad="REF"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="GND1">
<contactref element="U$1" pad="GND"/>
<contactref element="C2" pad="1"/>
<contactref element="U$7" pad="PAD"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="VE1"/>
<contactref element="U$1" pad="VO1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="VE2"/>
<contactref element="U$1" pad="VO2"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="VC1"/>
<contactref element="U$10" pad="PAD"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="II1"/>
<contactref element="U$9" pad="PAD"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="IO1"/>
<contactref element="U$11" pad="PAD"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="VC2"/>
<contactref element="U$3" pad="PAD"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="II2"/>
<contactref element="U$2" pad="PAD"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="OI2"/>
<contactref element="U$5" pad="PAD"/>
</signal>
<signal name="S$1">
<contactref element="U$1" pad="EE"/>
<contactref element="U$8" pad="PAD"/>
</signal>
<signal name="S$2">
<contactref element="U$6" pad="PAD"/>
<contactref element="U$1" pad="CC"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="REF"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="GND2">
<contactref element="U$17" pad="GND"/>
<contactref element="C3" pad="1"/>
<contactref element="U$23" pad="PAD"/>
</signal>
<signal name="N$16">
<contactref element="U$17" pad="VE1"/>
<contactref element="U$17" pad="VO1"/>
</signal>
<signal name="N$17">
<contactref element="U$17" pad="VE2"/>
<contactref element="U$17" pad="VO2"/>
</signal>
<signal name="N$18">
<contactref element="U$17" pad="VC1"/>
<contactref element="U$26" pad="PAD"/>
</signal>
<signal name="N$19">
<contactref element="U$17" pad="II1"/>
<contactref element="U$25" pad="PAD"/>
</signal>
<signal name="N$21">
<contactref element="U$17" pad="IO1"/>
<contactref element="U$27" pad="PAD"/>
</signal>
<signal name="N$22">
<contactref element="U$17" pad="VC2"/>
<contactref element="U$19" pad="PAD"/>
</signal>
<signal name="N$24">
<contactref element="U$17" pad="II2"/>
<contactref element="U$18" pad="PAD"/>
</signal>
<signal name="N$26">
<contactref element="U$17" pad="OI2"/>
<contactref element="U$21" pad="PAD"/>
</signal>
<signal name="S$3">
<contactref element="U$17" pad="EE"/>
<contactref element="U$24" pad="PAD"/>
</signal>
<signal name="S$4">
<contactref element="U$22" pad="PAD"/>
<contactref element="U$17" pad="CC"/>
</signal>
<signal name="N$27">
<contactref element="U$17" pad="REF"/>
<contactref element="C3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
