(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 15)
    (no_connects 0)
    (area 140.132999 77.648999 163.651001 156.031001)
    (thickness 1.6)
    (drawings 21)
    (tracks 63)
    (zones 0)
    (modules 11)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 40)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BZ1-Pad1)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 "Net-(Q1-Pad1)")
  (net 5 "Net-(Q1-Pad3)")
  (net 6 "Net-(Q2-Pad2)")
  (net 7 "Net-(R1-Pad1)")
  (net 8 "Net-(R1-Pad2)")
  (net 9 "Net-(J1-Pad1)")
  (net_class Default "To jest domyślna klasa połączeń."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(BZ1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net VCC)
  )
  (module myfootprint:MoistureSensor (layer F.Cu) (tedit 5A74A973)
    (at 151.892 131.572)
    (fp_text reference J1 (at 0 -22.86) (layer F.SilkS))
    (fp_text value Conn_01x02 (at -11.43 -3.81) (layer F.Fab))
    (pad 1 connect rect (at -7.62 0) (size 5 40) (layers F.Cu F.Mask)
      (net 9 "Net-(J1-Pad1)"))
    (pad 2 connect rect (at 7.62 0) (size 5 40) (layers F.Cu F.Mask)
      (net 3 VCC))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 144.272 90.932)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 1M (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buzzers_Beepers:Buzzer_12x9.5RM7.6 (layer F.Cu) (tedit 5A74A619)
    (at 159.004 86.36 180)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference BZ1 (at 4.064 0 180) (layer F.SilkS))
    (fp_text value Buzzer (at 3.8 7.4 180) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 180) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 180) (layer F.SilkS))
    (fp_text user %R (at 3.8 -4 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BZ1-Pad1)"))
    (pad 2 thru_hole circle (at 7.6 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Buzzers_Beepers.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A74A090)
    (at 142.748 84.328 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference Power1 (at 2.54 1.016 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 144.272 94.488)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 144.272 98.044)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 1M (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_VishaySpectrol_Econtrim-Type36T (layer F.Cu) (tedit 588234B0)
    (at 142.748 102.108 270)
    (descr "Potentiometer, Trimmer, Spectrol Type 36T, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer Trimmer Spectrol Type 36T Econtrim Rev A 02 Aug 2010 ")
    (fp_text reference RV1 (at 2.5 -7.05 270) (layer F.SilkS))
    (fp_text value 10K (at 2.5 2.05 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 -5 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A74A58E)
    (at 150.368 97.028 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value BC847 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A74A592)
    (at 154.94 97.028 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value BC847 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A74A596)
    (at 159.512 97.028 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value BC847 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BZ1-Pad1)"))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 155.956 105.156)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_text - (at 145.288 87.376) (layer F.SilkS))
  (gr_text + (at 142.748 87.376) (layer F.SilkS))
  (gr_text "THANKS TO THIS SMALL DEVICE \nYOU WILL NEVER FORGET TO \nWATER YOUR FLOWERS AGAIN" (at 151.384 111.252) (layer B.SilkS))
  (gr_text "HAPPY MAKING!" (at 159.512 133.096 90) (layer B.SilkS))
  (gr_text "THIS SITE TO THE GROUND >" (at 144.272 132.588 90) (layer B.SilkS))
  (gr_text "NIKODEM BARTNIK\n02.02.2018\nPROJECT: FLOTCHER V1\nNIKODEMBARTNIK.PL" (at 152.4 98.044) (layer B.SilkS))
  (gr_arc (start 151.892 119.38) (end 151.892 115.824) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151.892 119.38) (end 148.336 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.448 119.38) (end 155.448 151.892) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.336 151.892) (end 148.336 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 141.732 79.248) (end 140.208 79.248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.208 79.756) (end 140.208 79.248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162.052 79.248) (end 162.052 77.724) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.576 79.756) (end 163.576 79.248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.732 77.724) (end 162.052 77.724) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.576 151.892) (end 163.576 79.756) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.512 155.956) (end 163.576 151.892) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.448 151.892) (end 159.512 155.956) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.272 155.956) (end 148.336 151.892) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.208 151.892) (end 144.272 155.956) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.208 79.756) (end 140.208 151.892) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.255))
    (polygon
      (pts
        (xy 140.716 141.224) (xy 140.716 151.384) (xy 144.272 154.94) (xy 147.828 151.384) (xy 147.828 117.348)
        (xy 149.352 115.824) (xy 151.892 114.808) (xy 154.432 115.824) (xy 155.956 117.348) (xy 155.956 151.384)
        (xy 159.512 154.94) (xy 163.068 151.384) (xy 163.068 80.772) (xy 163.068 80.264) (xy 163.068 79.756)
        (xy 161.544 78.232) (xy 142.24 78.232) (xy 140.716 79.756)
      )
    )
  )
  (zone (net 3) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1) (thermal_bridge_width 0.255))
    (polygon
      (pts
        (xy 140.716 141.224) (xy 140.716 151.384) (xy 144.272 154.94) (xy 147.828 151.384) (xy 147.828 117.348)
        (xy 149.352 115.824) (xy 151.892 114.808) (xy 154.432 115.824) (xy 155.956 117.348) (xy 155.956 151.384)
        (xy 159.512 154.94) (xy 163.068 151.384) (xy 163.068 80.772) (xy 163.068 80.264) (xy 163.068 79.756)
        (xy 161.544 78.232) (xy 142.24 78.232) (xy 140.716 79.756)
      )
    )
  )
)
