<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="60.96" y2="0" width="0.2032" layer="20"/>
<wire x1="60.96" y1="0" x2="60.96" y2="27.94" width="0.2032" layer="20"/>
<wire x1="60.96" y1="27.94" x2="0" y2="27.94" width="0.2032" layer="20"/>
<wire x1="0" y1="27.94" x2="0" y2="0" width="0.2032" layer="20"/>
<text>T9A-30A/120V</text>
<text>GND</text>
<text>5V</text>
<text>LOAD</text>
<text>Relay Control PCB</text>
<text>Open</text>
<text>Normally</text>
<text>CTRL</text>
<text>Purple Squirrel</text>
<text>www.prplsqrl.com</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="AXIAL-0.3">
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="DIODE-1N4148">
</package>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="CREATIVE_COMMONS">
</package>
<package name="RELAY-T9A-2">
</package>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="Purplesquirrel_logo4">
<packages>
<package name="PURPLESQUIRREL_LOGO4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="SCREWTERMINAL-5MM-2" value="Load">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun" package="TO-92" value="2N3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="AXIAL-0.3" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="AXIAL-0.3" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$4" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$5" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="U$7" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="D1" library="SparkFun" package="DIODE-1N4148" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="AXIAL-0.3" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="SCREWTERMINAL-3.5MM-3" value=""/>
<element name="U6" library="SparkFun" package="RELAY-T9A-2" value="RELAYPTH3"/>
<element name="U$9" library="SparkFun" package="CREATIVE_COMMONS" value="CREATIVE_COMMONS"/>
<element name="U$12" library="SparkFun" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="U$1" library="Purplesquirrel_logo4" package="PURPLESQUIRREL_LOGO4" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="Q1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="RAW">
<contactref element="D1" pad="C"/>
<contactref element="LED1" pad="A"/>
<contactref element="JP2" pad="3"/>
<contactref element="U6" pad="COIL1"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="RELAY">
<contactref element="R2" pad="P$2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="LED1" pad="K"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="COIL">
<contactref element="Q1" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="R4" pad="P$1"/>
<contactref element="U6" pad="COIL2"/>
</signal>
<signal name="LOAD2">
<contactref element="JP1" pad="2"/>
<contactref element="U6" pad="NO"/>
</signal>
<signal name="LOAD1">
<contactref element="JP1" pad="1"/>
<contactref element="U6" pad="MAIN"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
