# Static Call Graph for image .\Obj\USART.axf

#<CALLGRAPH># ARM Linker, RVCT4.0 [Build 524]: Last Updated: Fri Aug 21 23:47:29 2009

### Maximum Stack Usage = 84 bytes + Unknown(Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ USART_Configuration1 ⇒ USART_Init ⇒ RCC_GetClocksFreq

### Function Pointers

- Reset_Handler
- NMIException
- HardFaultException
- MemManageException
- BusFaultException
- UsageFaultException
- SVCHandler
- DebugMonitor
- PendSVC
- SysTickHandler
- WWDG_IRQHandler
- PVD_IRQHandler
- TAMPER_IRQHandler
- RTC_IRQHandler
- FLASH_IRQHandler
- RCC_IRQHandler
- EXTI0_IRQHandler
- EXTI1_IRQHandler
- EXTI2_IRQHandler
- EXTI3_IRQHandler
- EXTI4_IRQHandler
- DMA1_Channel1_IRQHandler
- DMA1_Channel2_IRQHandler
- DMA1_Channel3_IRQHandler
- DMA1_Channel4_IRQHandler
- DMA1_Channel5_IRQHandler
- DMA1_Channel6_IRQHandler
- DMA1_Channel7_IRQHandler
- ADC1_2_IRQHandler
- USB_HP_CAN_TX_IRQHandler
- USB_LP_CAN_RX0_IRQHandler
- CAN_RX1_IRQHandler
- CAN_SCE_IRQHandler
- EXTI9_5_IRQHandler
- TIM1_BRK_IRQHandler
- TIM1_UP_IRQHandler
- TIM1_TRG_COM_IRQHandler
- TIM1_CC_IRQHandler
- TIM2_IRQHandler
- TIM3_IRQHandler
- TIM4_IRQHandler
- I2C1_EV_IRQHandler
- I2C1_ER_IRQHandler
- I2C2_EV_IRQHandler
- I2C2_ER_IRQHandler
- SPI1_IRQHandler
- SPI2_IRQHandler
- USART1_IRQHandler
- USART2_IRQHandler
- USART3_IRQHandler
- EXTI15_10_IRQHandler
- RTCAlarm_IRQHandler
- USBWakeUp_IRQHandler
- TIM8_BRK_IRQHandler
- TIM8_UP_IRQHandler
- TIM8_TRG_COM_IRQHandler
- TIM8_CC_IRQHandler
- ADC3_IRQHandler
- FSMC_IRQHandler
- SDIO_IRQHandler
- TIM5_IRQHandler
- SPI3_IRQHandler
- UART4_IRQHandler
- UART5_IRQHandler
- TIM6_IRQHandler
- TIM7_IRQHandler
- DMA2_Channel1_IRQHandler
- DMA2_Channel2_IRQHandler
- DMA2_Channel3_IRQHandler
- DMA2_Channel4_5_IRQHandler
- main
- __main
- fputc

### Global Symbols

__main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
[Address Reference Count : 1]

- stm32f10x_vector.o(.text)

_main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

_main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
[Calls]

- >> __scatterload

__main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
[Called By]

- >> __scatterload

_main_init (Thumb, 0 bytes, Stack size unknown bytes, entry7.o(.ARM.Collect$$$$00000007))

Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_vector.o(.text))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

__aeabi_uldivmod (Thumb, 90 bytes, Stack size 32 bytes, uldiv.o(.text), UNUSED)
[Calls]

- >> __aeabi_llsr
- >> __aeabi_llsl

[Called By]

- >> _printf_core

__scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
[Calls]

- >> __main_after_scatterload

[Called By]

- >> _main_scatterload

__scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

__aeabi_llsl (Thumb, 32 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
[Called By]

- >> __aeabi_uldivmod

_ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

__aeabi_llsr (Thumb, 30 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
[Called By]

- >> __aeabi_uldivmod

_ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

ADC1_2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.ADC1_2_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

ADC3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.ADC3_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

ADC_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_Cmd))
[Called By]

- >> main

ADC_DMACmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_DMACmd))
[Called By]

- >> main

ADC_GetCalibrationStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_GetCalibrationStatus))
[Called By]

- >> main

ADC_GetConversionValue (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_GetConversionValue))
[Called By]

- >> main

ADC_GetResetCalibrationStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_GetResetCalibrationStatus))
[Called By]

- >> main

ADC_Init (Thumb, 62 bytes, Stack size 12 bytes, stm32f10x_adc.o(i.ADC_Init))
[Stack]

- Max Depth = 12
- Call Chain = ADC_Init

[Called By]

- >> main

ADC_RegularChannelConfig (Thumb, 116 bytes, Stack size 16 bytes, stm32f10x_adc.o(i.ADC_RegularChannelConfig))
[Stack]

- Max Depth = 16
- Call Chain = ADC_RegularChannelConfig

[Called By]

- >> main

ADC_ResetCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_ResetCalibration))
[Called By]

- >> main

ADC_SoftwareStartConvCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_SoftwareStartConvCmd))
[Called By]

- >> main

ADC_StartCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(i.ADC_StartCalibration))
[Called By]

- >> main

BusFaultException (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFaultException))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

CAN_RX1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.CAN_RX1_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

CAN_SCE_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.CAN_SCE_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA1_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel1_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA1_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel2_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA1_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel3_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA1_Channel4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel4_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA1_Channel5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel5_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA1_Channel6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel6_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA1_Channel7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel7_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA2_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel1_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA2_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel2_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA2_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel3_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA2_Channel4_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel4_5_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

DMA_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_dma.o(i.DMA_Cmd))
[Called By]

- >> main

DMA_DeInit (Thumb, 210 bytes, Stack size 0 bytes, stm32f10x_dma.o(i.DMA_DeInit))
[Called By]

- >> main

DMA_Init (Thumb, 58 bytes, Stack size 16 bytes, stm32f10x_dma.o(i.DMA_Init))
[Stack]

- Max Depth = 16
- Call Chain = DMA_Init

[Called By]

- >> main

DebugMonitor (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMonitor))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

EXTI0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI0_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

EXTI15_10_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI15_10_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

EXTI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI1_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

EXTI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI2_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

EXTI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI3_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

EXTI4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI4_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

EXTI9_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI9_5_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

FLASH_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.FLASH_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

FLASH_PrefetchBufferCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_PrefetchBufferCmd))
[Called By]

- >> RCC_Configuration

FLASH_SetLatency (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_SetLatency))
[Called By]

- >> RCC_Configuration

FSMC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.FSMC_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

GPIO_Configuration (Thumb, 74 bytes, Stack size 8 bytes, main.o(i.GPIO_Configuration))
[Stack]

- Max Depth = 28
- Call Chain = GPIO_Configuration ⇒ GPIO_Init

[Calls]

- >> GPIO_Init

[Called By]

- >> main

GPIO_Init (Thumb, 160 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_Init))
[Stack]

- Max Depth = 20
- Call Chain = GPIO_Init

[Called By]

- >> GPIO_Configuration

HardFaultException (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFaultException))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

I2C1_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C1_ER_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

I2C1_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C1_EV_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

I2C2_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C2_ER_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

I2C2_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C2_EV_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

MemManageException (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManageException))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

NMIException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMIException))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

NVIC_Configuration (Thumb, 22 bytes, Stack size 8 bytes, main.o(i.NVIC_Configuration))
[Stack]

- Max Depth = 8
- Call Chain = NVIC_Configuration

[Calls]

- >> NVIC_SetVectorTable
- >> NVIC_PriorityGroupConfig

[Called By]

- >> main

NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_nvic.o(i.NVIC_PriorityGroupConfig))
[Called By]

- >> NVIC_Configuration

NVIC_SetVectorTable (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_nvic.o(i.NVIC_SetVectorTable))
[Called By]

- >> NVIC_Configuration

PVD_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PVD_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

PendSVC (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSVC))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

RCC_AHBPeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_AHBPeriphClockCmd))
[Called By]

- >> RCC_Configuration

RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
[Called By]

- >> RCC_Configuration

RCC_Configuration (Thumb, 138 bytes, Stack size 8 bytes, main.o(i.RCC_Configuration))
[Stack]

- Max Depth = 20
- Call Chain = RCC_Configuration ⇒ RCC_WaitForHSEStartUp

[Calls]

- >> RCC_WaitForHSEStartUp
- >> RCC_SYSCLKConfig
- >> RCC_PLLConfig
- >> RCC_PLLCmd
- >> RCC_PCLK2Config
- >> RCC_PCLK1Config
- >> RCC_HSEConfig
- >> RCC_HCLKConfig
- >> RCC_GetSYSCLKSource
- >> RCC_GetFlagStatus
- >> RCC_DeInit
- >> RCC_APB2PeriphClockCmd
- >> RCC_AHBPeriphClockCmd
- >> FLASH_SetLatency
- >> FLASH_PrefetchBufferCmd

[Called By]

- >> main

RCC_DeInit (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_DeInit))
[Called By]

- >> RCC_Configuration

RCC_GetClocksFreq (Thumb, 132 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
[Stack]

- Max Depth = 12
- Call Chain = RCC_GetClocksFreq

[Called By]

- >> USART_Init

RCC_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetFlagStatus))
[Called By]

- >> RCC_WaitForHSEStartUp
- >> RCC_Configuration

RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetSYSCLKSource))
[Called By]

- >> RCC_Configuration

RCC_HCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HCLKConfig))
[Called By]

- >> RCC_Configuration

RCC_HSEConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HSEConfig))
[Called By]

- >> RCC_Configuration

RCC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RCC_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

RCC_PCLK1Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK1Config))
[Called By]

- >> RCC_Configuration

RCC_PCLK2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK2Config))
[Called By]

- >> RCC_Configuration

RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLCmd))
[Called By]

- >> RCC_Configuration

RCC_PLLConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLConfig))
[Called By]

- >> RCC_Configuration

RCC_SYSCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_SYSCLKConfig))
[Called By]

- >> RCC_Configuration

RCC_WaitForHSEStartUp (Thumb, 46 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_WaitForHSEStartUp))
[Stack]

- Max Depth = 12
- Call Chain = RCC_WaitForHSEStartUp

[Calls]

- >> RCC_GetFlagStatus

[Called By]

- >> RCC_Configuration

RTCAlarm_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RTCAlarm_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

RTC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RTC_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

SDIO_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SDIO_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

SPI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI1_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

SPI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI2_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

SPI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI3_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

SVCHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVCHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

SysTickHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTickHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TAMPER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TAMPER_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM1_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_BRK_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM1_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_CC_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM1_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_TRG_COM_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM1_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_UP_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM2_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM3_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM4_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM5_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM6_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM7_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM8_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_BRK_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM8_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_CC_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM8_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_TRG_COM_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

TIM8_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_UP_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

UART4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UART4_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

UART5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UART5_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

USART1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART1_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

USART2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART2_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

USART3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART3_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

USART_ClockInit (Thumb, 30 bytes, Stack size 12 bytes, stm32f10x_usart.o(i.USART_ClockInit))
[Stack]

- Max Depth = 12
- Call Chain = USART_ClockInit

[Called By]

- >> USART_Configuration1

USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
[Called By]

- >> USART_Configuration1

USART_Configuration1 (Thumb, 86 bytes, Stack size 32 bytes, main.o(i.USART_Configuration1))
[Stack]

- Max Depth = 76
- Call Chain = USART_Configuration1 ⇒ USART_Init ⇒ RCC_GetClocksFreq

[Calls]

- >> USART_Init
- >> USART_Cmd
- >> USART_ClockInit

[Called By]

- >> main

USART_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
[Called By]

- >> fputc

USART_Init (Thumb, 130 bytes, Stack size 32 bytes, stm32f10x_usart.o(i.USART_Init))
[Stack]

- Max Depth = 44
- Call Chain = USART_Init ⇒ RCC_GetClocksFreq

[Calls]

- >> RCC_GetClocksFreq

[Called By]

- >> USART_Configuration1

USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
[Called By]

- >> fputc

USBWakeUp_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USBWakeUp_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

USB_HP_CAN_TX_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USB_HP_CAN_TX_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

USB_LP_CAN_RX0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USB_LP_CAN_RX0_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

UsageFaultException (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFaultException))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

WWDG_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.WWDG_IRQHandler))
[Address Reference Count : 1]

- stm32f10x_vector.o(RESET)

__0printf$8 (Thumb, 22 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)
[Calls]

- >> _printf_core

__1printf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)

__2printf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8))
[Stack]

- Max Depth = 24
- Call Chain = __2printf

[Called By]

- >> main

__scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

__scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

__scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

fputc (Thumb, 32 bytes, Stack size 16 bytes, main.o(i.fputc))
[Stack]

- Max Depth = 16
- Call Chain = fputc

[Calls]

- >> USART_SendData
- >> USART_GetFlagStatus

[Address Reference Count : 1]

- printf8.o(i.__0printf$8)

main (Thumb, 280 bytes, Stack size 8 bytes, main.o(i.main))
[Stack]

- Max Depth = 84
- Call Chain = main ⇒ USART_Configuration1 ⇒ USART_Init ⇒ RCC_GetClocksFreq

[Calls]

- >> DMA_Init
- >> DMA_DeInit
- >> DMA_Cmd
- >> ADC_StartCalibration
- >> ADC_SoftwareStartConvCmd
- >> ADC_ResetCalibration
- >> ADC_RegularChannelConfig
- >> ADC_Init
- >> ADC_GetResetCalibrationStatus
- >> ADC_GetConversionValue
- >> ADC_GetCalibrationStatus
- >> ADC_DMACmd
- >> ADC_Cmd
- >> USART_Configuration1
- >> RCC_Configuration
- >> NVIC_Configuration
- >> GPIO_Configuration
- >> __2printf

[Address Reference Count : 1]

- entry7.o(.ARM.Collect$$$$00000007)

### Local Symbols

_printf_core (Thumb, 1102 bytes, Stack size 128 bytes, printf8.o(i._printf_core), UNUSED)
[Calls]

- >> __aeabi_uldivmod
- >> _printf_pre_padding
- >> _printf_post_padding

[Called By]

- >> __0printf$8

_printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf8.o(i._printf_post_padding), UNUSED)
[Called By]

- >> _printf_core

_printf_pre_padding (Thumb, 44 bytes, Stack size 24 bytes, printf8.o(i._printf_pre_padding), UNUSED)
[Called By]

- >> _printf_core

### Undefined Global Symbols