# Static Call Graph for image .\Obj\STM3210E-EVAL.axf

#<CALLGRAPH># ARM Linker, RVCT4.0 [Build 524]: Last Updated: Wed Aug 19 22:36:27 2009

### Maximum Stack Usage = 68 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ USART_Init ⇒ RCC_GetClocksFreq

### Mutually Recursive functions

- BusFaultException ⇒ BusFaultException
- HardFaultException ⇒ HardFaultException
- MemManageException ⇒ MemManageException
- UsageFaultException ⇒ UsageFaultException

  ### Function Pointers

  - Reset_Handler
  - NMIException
  - HardFaultException
  - MemManageException
  - BusFaultException
  - UsageFaultException
  - SVCHandler
  - DebugMonitor
  - PendSVC
  - SysTickHandler
  - WWDG_IRQHandler
  - PVD_IRQHandler
  - TAMPER_IRQHandler
  - RTC_IRQHandler
  - FLASH_IRQHandler
  - RCC_IRQHandler
  - EXTI0_IRQHandler
  - EXTI1_IRQHandler
  - EXTI2_IRQHandler
  - EXTI3_IRQHandler
  - EXTI4_IRQHandler
  - DMA1_Channel1_IRQHandler
  - DMA1_Channel2_IRQHandler
  - DMA1_Channel3_IRQHandler
  - DMA1_Channel4_IRQHandler
  - DMA1_Channel5_IRQHandler
  - DMA1_Channel6_IRQHandler
  - DMA1_Channel7_IRQHandler
  - ADC1_2_IRQHandler
  - USB_HP_CAN_TX_IRQHandler
  - USB_LP_CAN_RX0_IRQHandler
  - CAN_RX1_IRQHandler
  - CAN_SCE_IRQHandler
  - EXTI9_5_IRQHandler
  - TIM1_BRK_IRQHandler
  - TIM1_UP_IRQHandler
  - TIM1_TRG_COM_IRQHandler
  - TIM1_CC_IRQHandler
  - TIM2_IRQHandler
  - TIM3_IRQHandler
  - TIM4_IRQHandler
  - I2C1_EV_IRQHandler
  - I2C1_ER_IRQHandler
  - I2C2_EV_IRQHandler
  - I2C2_ER_IRQHandler
  - SPI1_IRQHandler
  - SPI2_IRQHandler
  - USART1_IRQHandler
  - USART2_IRQHandler
  - USART3_IRQHandler
  - EXTI15_10_IRQHandler
  - RTCAlarm_IRQHandler
  - USBWakeUp_IRQHandler
  - TIM8_BRK_IRQHandler
  - TIM8_UP_IRQHandler
  - TIM8_TRG_COM_IRQHandler
  - TIM8_CC_IRQHandler
  - ADC3_IRQHandler
  - FSMC_IRQHandler
  - SDIO_IRQHandler
  - TIM5_IRQHandler
  - SPI3_IRQHandler
  - UART4_IRQHandler
  - UART5_IRQHandler
  - TIM6_IRQHandler
  - TIM7_IRQHandler
  - DMA2_Channel1_IRQHandler
  - DMA2_Channel2_IRQHandler
  - DMA2_Channel3_IRQHandler
  - DMA2_Channel4_5_IRQHandler
  - main
  - __main

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry7.o(.ARM.Collect$$$$00000007))

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_vector.o(.text))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  ADC1_2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.ADC1_2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  ADC3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.ADC3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  Buffercmp (Thumb, 34 bytes, Stack size 8 bytes, main.o(i.Buffercmp))
  [Stack]

  - Max Depth = 8
  - Call Chain = Buffercmp
  [Called By]
  - >> main

  BusFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFaultException))
  [Calls]

  - >> BusFaultException
  [Called By]
  - >> BusFaultException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.CAN_RX1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.CAN_SCE_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel6_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA1_Channel7_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DMA2_Channel4_5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  DebugMonitor (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMonitor))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI0_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI15_10_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.EXTI9_5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  FLASH_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.FLASH_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  FLASH_PrefetchBufferCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_PrefetchBufferCmd))
  [Called By]

  - >> RCC_Configuration

  FLASH_SetLatency (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_SetLatency))
  [Called By]

  - >> RCC_Configuration

  FSMC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.FSMC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  GPIO_Configuration (Thumb, 80 bytes, Stack size 16 bytes, main.o(i.GPIO_Configuration))
  [Stack]

  - Max Depth = 36
  - Call Chain = GPIO_Configuration ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  [Called By]
  - >> main

  GPIO_Init (Thumb, 160 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> GPIO_Configuration

  HardFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFaultException))
  [Calls]

  - >> HardFaultException
  [Called By]
  - >> HardFaultException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C1_ER_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C1_EV_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C2_ER_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.I2C2_EV_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  MemManageException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManageException))
  [Calls]

  - >> MemManageException
  [Called By]
  - >> MemManageException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  NMIException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMIException))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  NVIC_Configuration (Thumb, 66 bytes, Stack size 16 bytes, main.o(i.NVIC_Configuration))
  [Stack]

  - Max Depth = 36
  - Call Chain = NVIC_Configuration ⇒ NVIC_Init
  [Calls]
  - >> NVIC_SetVectorTable
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  [Called By]
  - >> main

  NVIC_Init (Thumb, 116 bytes, Stack size 20 bytes, stm32f10x_nvic.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = NVIC_Init
  [Called By]
  - >> NVIC_Configuration

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_nvic.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> NVIC_Configuration

  NVIC_SetVectorTable (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_nvic.o(i.NVIC_SetVectorTable))
  [Called By]

  - >> NVIC_Configuration

  PVD_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PVD_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  PendSVC (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSVC))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> RCC_Configuration

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> RCC_Configuration

  RCC_Configuration (Thumb, 122 bytes, Stack size 8 bytes, main.o(i.RCC_Configuration))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_Configuration ⇒ RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_WaitForHSEStartUp
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLConfig
  - >> RCC_PLLCmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HSEConfig
  - >> RCC_HCLKConfig
  - >> RCC_GetSYSCLKSource
  - >> RCC_GetFlagStatus
  - >> RCC_DeInit
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> FLASH_SetLatency
  - >> FLASH_PrefetchBufferCmd
  [Called By]
  - >> main

  RCC_DeInit (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_DeInit))
  [Called By]

  - >> RCC_Configuration

  RCC_GetClocksFreq (Thumb, 132 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RCC_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetFlagStatus))
  [Called By]

  - >> RCC_WaitForHSEStartUp
  - >> RCC_Configuration

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_GetSYSCLKSource))
  [Called By]

  - >> RCC_Configuration

  RCC_HCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HCLKConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_HSEConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_HSEConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RCC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  RCC_PCLK1Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK1Config))
  [Called By]

  - >> RCC_Configuration

  RCC_PCLK2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PCLK2Config))
  [Called By]

  - >> RCC_Configuration

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLCmd))
  [Called By]

  - >> RCC_Configuration

  RCC_PLLConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_PLLConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_SYSCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_SYSCLKConfig))
  [Called By]

  - >> RCC_Configuration

  RCC_WaitForHSEStartUp (Thumb, 46 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_WaitForHSEStartUp))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> RCC_Configuration

  RTCAlarm_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RTCAlarm_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  RTC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.RTC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SDIO_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SDIO_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SPI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI1_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SPI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SPI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SPI3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SVCHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVCHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  SysTickHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTickHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TAMPER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TAMPER_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_BRK_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_CC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_TRG_COM_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM1_UP_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM2_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM6_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM7_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_BRK_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_CC_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_TRG_COM_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.TIM8_UP_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  UART4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UART4_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  UART5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UART5_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USART1_IRQHandler (Thumb, 120 bytes, Stack size 16 bytes, stm32f10x_it.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_SendData
  - >> USART_ReceiveData
  - >> USART_ITConfig
  - >> USART_GetITStatus
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  USART2_IRQHandler (Thumb, 120 bytes, Stack size 16 bytes, stm32f10x_it.o(i.USART2_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = USART2_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_SendData
  - >> USART_ReceiveData
  - >> USART_ITConfig
  - >> USART_GetITStatus
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  USART3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USART3_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> main

  USART_GetITStatus (Thumb, 62 bytes, Stack size 16 bytes, stm32f10x_usart.o(i.USART_GetITStatus))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART2_IRQHandler
  - >> USART1_IRQHandler

  USART_ITConfig (Thumb, 48 bytes, Stack size 8 bytes, stm32f10x_usart.o(i.USART_ITConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ITConfig
  [Called By]
  - >> main
  - >> USART2_IRQHandler
  - >> USART1_IRQHandler

  USART_Init (Thumb, 130 bytes, Stack size 32 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 44
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> main

  USART_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ReceiveData))
  [Called By]

  - >> USART2_IRQHandler
  - >> USART1_IRQHandler

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> USART2_IRQHandler
  - >> USART1_IRQHandler

  USBWakeUp_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USBWakeUp_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USB_HP_CAN_TX_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USB_HP_CAN_TX_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  USB_LP_CAN_RX0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.USB_LP_CAN_RX0_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  UsageFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFaultException))
  [Calls]

  - >> UsageFaultException
  [Called By]
  - >> UsageFaultException
  [Address Reference Count : 1]
  - stm32f10x_vector.o(RESET)

  WWDG_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.WWDG_IRQHandler))
  [Address Reference Count : 1]

  - stm32f10x_vector.o(RESET)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 170 bytes, Stack size 24 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 68
  - Call Chain = main ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_Cmd
  - >> RCC_Configuration
  - >> NVIC_Configuration
  - >> GPIO_Configuration
  - >> Buffercmp
  - >> USART_ITConfig
  [Address Reference Count : 1]
  - entry7.o(.ARM.Collect$$$$00000007)

  ### Local Symbols

  ### Undefined Global Symbols