Par Statistics
Total Non-vccgnd Signals=72
Total Non-vccgnd Design Pins=299
Total Non-vccgnd Conns=299
Total Non-vccgnd Timing Constrained Conns=270
Phase 1 CPU=17.3 sec
Phase 2 CPU=17.6 sec
Phase 3 CPU=17.8 sec
Phase 4 CPU=22.5 sec
Phase 5 CPU=22.6 sec
Phase 6 CPU=22.6 sec
Phase 7 CPU=22.6 sec
Phase 8 CPU=22.6 sec
Phase 9 CPU=22.7 sec
AvgWirelenPerPin Fanout 1=3.0
AvgWirelenPerPin Fanout 2=14.0
AvgWirelenPerPin Fanout 3=1.0
AvgWirelenPerPin Fanout 4=13.3
AvgWirelenPerPin Fanout 10=7.3
AvgWirelenPerPin Fanout 50=2.8
AvgWirelenPerPin Fanout 100=0.0
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.0047