The Ring is 72” diameter with a wall 5” high to catch the paint that will be thrown from the platform. Using Pi D , 3.1417 x 72 = 229.34” length of wall. 3 pieces 80” or 4 pieces 60” with overlap for assembly. Corogate plastic is easier to bend after it has heated up in the sun and staked or pinned to the desired shape. The ends can be joined with zip ties and hot melt glue as shown. Make 4 filler panels as needed to catch paine.