<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.75" y2="0" width="0.2032" layer="20"/>
<wire x1="31.75" y1="0" x2="31.75" y2="31.75" width="0.2032" layer="20"/>
<wire x1="31.75" y1="31.75" x2="0" y2="31.75" width="0.2032" layer="20"/>
<wire x1="0" y1="31.75" x2="0" y2="0" width="0.2032" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>OFF</text>
<text>ON</text>
<text>POWER</text>
<text>PTC</text>
<text>6-3-08</text>
<text>3.3V</text>
<text>5V</text>
<text>-</text>
<text>+</text>
<text>NC</text>
<text>6-12VDC</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SWITCH-SPST">
</package>
<package name="TO220-ADJ">
</package>
<package name="PTC">
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="1X02">
</package>
<package name="DIODE-0.4">
</package>
<package name="AXIAL-0.3">
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="CAP-PTH-SMALL2">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-Nate">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="Purplesquirrel_logo4">
<packages>
<package name="PURPLESQUIRREL_LOGO4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="SparkFun" package="SWITCH-SPST" value="On/Off"/>
<element name="R2" library="SparkFun" package="AXIAL-0.3" value="390">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="CPOL-RADIAL-100UF-25V" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="AXIAL-0.3" value="240">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="AXIAL-0.3" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-Nate" package="LED5MM" value="Power"/>
<element name="C3" library="SparkFun" package="CAP-PTH-SMALL2" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun" package="TO220-ADJ" value="LM317"/>
<element name="F1" library="SparkFun" package="PTC" value="500mA"/>
<element name="JP1" library="SparkFun" package="1X01" value=""/>
<element name="JP2" library="SparkFun" package="1X01" value=""/>
<element name="JP3" library="SparkFun" package="1X01" value=""/>
<element name="JP4" library="SparkFun" package="1X01" value=""/>
<element name="J1" library="SparkFun" package="POWER_JACK_PTH" value="POWER_JACKPTH"/>
<element name="JP5" library="SparkFun" package="1X02" value=""/>
<element name="D1" library="SparkFun" package="DIODE-0.4" value="1N4001"/>
<element name="S2" library="SparkFun" package="SWITCH-SPST" value="Voltage"/>
<element name="R3" library="SparkFun" package="AXIAL-0.3" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Purplesquirrel_logo4" package="PURPLESQUIRREL_LOGO4" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="LED2" pad="K"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="JP5" pad="2"/>
<contactref element="R3" pad="P$1"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="U1" pad="ADJ"/>
</signal>
<signal name="N$8">
<contactref element="LED2" pad="A"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="RAW">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="IN"/>
<contactref element="F1" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="P$2"/>
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="P$2"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="OUT"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="F1" pad="P$1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="PWR"/>
<contactref element="S1" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="P$1"/>
<contactref element="R3" pad="P$2"/>
<contactref element="S2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
