NeoPixel Driver artwork. Note this is the trackside view and the size (excluding the small boxes on the corners should be width 0.7” and height 1.9”. Adjust if necessary by changing the picture size (right click and Size and Position). . The switch locating holes are 0.7mm, the capacitor 0.7 or 0.8mm, holes to the Arduino 0.7 to 0.9mm (use latter if using pinstrip pins to connect), holes for leads to Led strip 1.2mm.

