**Breakout Board Materials**

1. PNG breakout board File (Found in the Breakout Board Process Step)
2. 12x 14 Double Sided Copper Clad Laminate PCB Circuit Board
3. Transfer Paper

<https://www.walmart.com/ip/EASTMAN-KODAK-High-Gloss-Ultra-Premium-Photo-Paper-4-x-6-20-Sheets-per-Pack/21424578>

1. Clothes Iron – to transfer image to Copper
2. Rubber gloves
3. Brillo pad
4. Scotch tape
5. Ferric chloride - For etching
6. Drill and 1/4” drill bit – to drill hole in copper board
7. String - to tie through hole