**Handle Materials**

1. 1 sheet of polystyrene foam

<https://www.lowes.com/pd/Dow-Common-0-55-in-x-4-ft-x-8-ft-Actual-0-55-in-x-4-ft-x-8-ft-Residential-Sheathing-Square-Edge-R5-Faced-Polystyrene-Foam-Board-Insulation-with-Sound-Barrier/1000183057>

1. Loctite Spray Adhesive High Performance 200

<http://www.homedepot.com/p/Loctite-13-5-oz-High-Performance-Spray-Adhesive-1408028/202365672>

1. Mod podge with gloss finish

<https://www.walmart.com/ip/Mod-Podge-Gloss-16-oz/17472598>

1. Foam Paint Brushes (to apply Mod Podge)

<https://www.walmart.com/ip/Linzer-A8509-Foam-Brush-Set-9-Piece/47651721>

1. Black Spray Plasti Dip

<https://www.walmart.com/ip/Plasti-Dip-Aerosol-Navy-Blue/165076369>

1. X-acto
2. Hot glue & glue sticks
3. 80 & 150 Grit sand paper

<https://www.walmart.com/ip/Grizzly-H9393-Super-Flex-80-Grit-Sandpaper-4-pk./48094822>

<https://www.walmart.com/ip/SUPER-FLEX-150-GRIT-SANDPAPER/48095128>

1. Combination Rasp

<https://www.lowes.com/pd/Kobalt-8-in-File/4307531>