TowerPro MG996R Servo

Specifications

|  |  |
| --- | --- |
| Modulation: | Digital |
| Torque: | **4.8V:** 130.54 oz-in (9.40 kg-cm)**6.0V:** 152.76 oz-in (11.00 kg-cm) |
| Speed: | **4.8V:** 0.19 sec/60°**6.0V:** 0.15 sec/60° |
| Weight: | 1.94 oz (55.0 g) |
| Dimensions: | **Length:**1.60 in (40.7 mm)**Width:**0.78 in (19.7 mm)**Height:**1.69 in (42.9 mm)  |
| Motor Type: | ([add](http://www.servodatabase.com/add-data?make=towerpro&model=mg996r)) |
| Gear Type: | Metal |
| Rotation/Support: | Dual Bearings  |
| Rotational Range: | ([add](http://www.servodatabase.com/add-data?make=towerpro&model=mg996r)) |
| Pulse Cycle: | 1 ms |
| Pulse Width: | ([add](http://www.servodatabase.com/add-data?make=towerpro&model=mg996r)) |
| Connector Type: | JR |



|  |  |
| --- | --- |
| Brand: | TowerPro |
| Product Number: | ([add](http://www.servodatabase.com/add-data?make=towerpro&model=mg996r)) |
| Typical Price: | 10.50 USD |