<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50" y2="0" width="0.1524" layer="20"/>
<wire x1="50" y1="0" x2="50" y2="50" width="0.1524" layer="20"/>
<wire x1="50" y1="50" x2="0" y2="50" width="0.1524" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0.1524" layer="20"/>
<hole x="48.006" y="2.032" drill="3"/>
<hole x="1.905" y="48.133" drill="3"/>
<hole x="1.524" y="1.36525" drill="1"/>
<text>G</text>
<text>V</text>
<text>L</text>
<text>R</text>
<text>Tiny
LoL
Leaf</text>
<hole x="1.524" y="34.544" drill="1"/>
<text>G</text>
<text>V</text>
<text>L</text>
<text>R</text>
<text>Tiny
LoL
Leaf</text>
<hole x="1.524" y="18.034" drill="1"/>
<text>G</text>
<text>V</text>
<text>L</text>
<text>R</text>
<text>Tiny
LoL
Leaf</text>
<hole x="34.544" y="1.36525" drill="1"/>
<text>G</text>
<text>V</text>
<text>L</text>
<text>R</text>
<text>Tiny
LoL
Leaf</text>
<hole x="34.544" y="34.544" drill="1"/>
<text>G</text>
<text>V</text>
<text>L</text>
<text>R</text>
<text>Tiny
LoL
Leaf</text>
<hole x="34.544" y="18.034" drill="1"/>
<text>G</text>
<text>V</text>
<text>L</text>
<text>R</text>
<text>Tiny
LoL
Leaf</text>
<hole x="18.034" y="1.524" drill="1"/>
<text>G</text>
<text>V</text>
<text>L</text>
<text>R</text>
<text>Tiny
LoL
Leaf</text>
<hole x="18.034" y="34.70275" drill="1"/>
<text>G</text>
<text>V</text>
<text>L</text>
<text>R</text>
<text>Tiny
LoL
Leaf</text>
<hole x="18.034" y="18.19275" drill="1"/>
<text>G</text>
<text>V</text>
<text>L</text>
<text>R</text>
<text>Tiny
LoL
Leaf</text>
</plain>
<libraries>
<library name="LoL Clock">
<description>Generated from &lt;b&gt;LoL Clock Tunes-210_09_mini.brd&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="LOL-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="PAD_1.27X2.54_LEAF">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ_MCU">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="L172" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L173" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L174" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L175" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L176" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L177" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L178" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L179" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L180" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L181" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L182" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L183" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD9" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD10" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U6" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD11" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD12" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="L13" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L14" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L15" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L16" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L17" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L18" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L19" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L20" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L21" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L22" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L23" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L24" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD13" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD14" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U2" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD15" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD16" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="L37" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L38" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L39" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L40" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L41" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L42" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L43" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L44" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L45" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L46" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L47" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L48" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD21" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD22" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U4" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD23" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD24" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="L1" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L2" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L3" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L4" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L5" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L6" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L7" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L8" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L9" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L10" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L11" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L12" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD1" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD2" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U1" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD3" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD4" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="L25" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L26" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L27" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L28" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L29" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L30" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L31" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L32" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L33" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L34" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L35" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L36" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD5" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD6" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U3" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD7" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD8" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="L49" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L50" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L51" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L52" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L53" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L54" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L55" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L56" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L57" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L58" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L59" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L60" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD17" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD18" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U5" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD19" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD20" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="L61" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L62" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L63" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L64" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L65" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L66" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L67" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L68" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L69" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L70" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L71" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L72" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD25" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD26" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U7" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD27" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD28" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="L73" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L74" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L75" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L76" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L77" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L78" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L79" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L80" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L81" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L82" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L83" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L84" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD29" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD30" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U8" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD31" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD32" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="L85" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L86" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L87" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L88" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L89" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L90" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L91" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L92" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L93" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L94" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L95" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L96" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD33" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD34" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U9" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD35" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD36" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
</elements>
<signals>
<signal name="D50">
<contactref element="L174" pad="A"/>
<contactref element="L177" pad="A"/>
<contactref element="L180" pad="A"/>
<contactref element="L181" pad="C"/>
<contactref element="L182" pad="C"/>
<contactref element="L183" pad="C"/>
<contactref element="U6" pad="7"/>
</signal>
<signal name="D51">
<contactref element="L172" pad="A"/>
<contactref element="L175" pad="C"/>
<contactref element="L176" pad="C"/>
<contactref element="L177" pad="C"/>
<contactref element="L179" pad="A"/>
<contactref element="L182" pad="A"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="D52">
<contactref element="L173" pad="A"/>
<contactref element="L178" pad="C"/>
<contactref element="L176" pad="A"/>
<contactref element="L179" pad="C"/>
<contactref element="L180" pad="C"/>
<contactref element="L183" pad="A"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="GND13">
<contactref element="PAD9" pad="1"/>
<contactref element="U6" pad="4"/>
</signal>
<signal name="+5V7">
<contactref element="PAD10" pad="1"/>
<contactref element="U6" pad="8"/>
</signal>
<signal name="SDA2">
<contactref element="U6" pad="5"/>
<contactref element="PAD12" pad="1"/>
</signal>
<signal name="D53">
<contactref element="L172" pad="C"/>
<contactref element="L175" pad="A"/>
<contactref element="L173" pad="C"/>
<contactref element="L178" pad="A"/>
<contactref element="L174" pad="C"/>
<contactref element="L181" pad="A"/>
<contactref element="U6" pad="6"/>
</signal>
<signal name="SCL4">
<contactref element="U6" pad="1"/>
<contactref element="PAD11" pad="1"/>
</signal>
<signal name="N$6">
</signal>
<signal name="D5">
<contactref element="L15" pad="A"/>
<contactref element="L18" pad="A"/>
<contactref element="L21" pad="A"/>
<contactref element="L22" pad="C"/>
<contactref element="L23" pad="C"/>
<contactref element="L24" pad="C"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="D6">
<contactref element="L13" pad="A"/>
<contactref element="L16" pad="C"/>
<contactref element="L17" pad="C"/>
<contactref element="L18" pad="C"/>
<contactref element="L20" pad="A"/>
<contactref element="L23" pad="A"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="D7">
<contactref element="L14" pad="A"/>
<contactref element="L19" pad="C"/>
<contactref element="L17" pad="A"/>
<contactref element="L20" pad="C"/>
<contactref element="L21" pad="C"/>
<contactref element="L24" pad="A"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="GND2">
<contactref element="PAD13" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="+5V2">
<contactref element="PAD14" pad="1"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="SDA4">
<contactref element="U2" pad="5"/>
<contactref element="PAD16" pad="1"/>
</signal>
<signal name="D8">
<contactref element="L13" pad="C"/>
<contactref element="L16" pad="A"/>
<contactref element="L14" pad="C"/>
<contactref element="L19" pad="A"/>
<contactref element="L15" pad="C"/>
<contactref element="L22" pad="A"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="SCL2">
<contactref element="U2" pad="1"/>
<contactref element="PAD15" pad="1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="D13">
<contactref element="L39" pad="A"/>
<contactref element="L42" pad="A"/>
<contactref element="L45" pad="A"/>
<contactref element="L46" pad="C"/>
<contactref element="L47" pad="C"/>
<contactref element="L48" pad="C"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="D14">
<contactref element="L37" pad="A"/>
<contactref element="L40" pad="C"/>
<contactref element="L41" pad="C"/>
<contactref element="L42" pad="C"/>
<contactref element="L44" pad="A"/>
<contactref element="L47" pad="A"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="D15">
<contactref element="L38" pad="A"/>
<contactref element="L43" pad="C"/>
<contactref element="L41" pad="A"/>
<contactref element="L44" pad="C"/>
<contactref element="L45" pad="C"/>
<contactref element="L48" pad="A"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="GND4">
<contactref element="PAD21" pad="1"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="+5V4">
<contactref element="PAD22" pad="1"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="SDA6">
<contactref element="U4" pad="5"/>
<contactref element="PAD24" pad="1"/>
</signal>
<signal name="D16">
<contactref element="L37" pad="C"/>
<contactref element="L40" pad="A"/>
<contactref element="L38" pad="C"/>
<contactref element="L43" pad="A"/>
<contactref element="L39" pad="C"/>
<contactref element="L46" pad="A"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="SCL6">
<contactref element="U4" pad="1"/>
<contactref element="PAD23" pad="1"/>
</signal>
<signal name="N$5">
</signal>
<signal name="D1">
<contactref element="L3" pad="A"/>
<contactref element="L6" pad="A"/>
<contactref element="L9" pad="A"/>
<contactref element="L10" pad="C"/>
<contactref element="L11" pad="C"/>
<contactref element="L12" pad="C"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="D2">
<contactref element="L1" pad="A"/>
<contactref element="L4" pad="C"/>
<contactref element="L5" pad="C"/>
<contactref element="L6" pad="C"/>
<contactref element="L8" pad="A"/>
<contactref element="L11" pad="A"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="D3">
<contactref element="L2" pad="A"/>
<contactref element="L7" pad="C"/>
<contactref element="L5" pad="A"/>
<contactref element="L8" pad="C"/>
<contactref element="L9" pad="C"/>
<contactref element="L12" pad="A"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="GND1">
<contactref element="PAD1" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="+5V1">
<contactref element="PAD2" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="SDA1">
<contactref element="U1" pad="5"/>
<contactref element="PAD4" pad="1"/>
</signal>
<signal name="D4">
<contactref element="L1" pad="C"/>
<contactref element="L4" pad="A"/>
<contactref element="L2" pad="C"/>
<contactref element="L7" pad="A"/>
<contactref element="L3" pad="C"/>
<contactref element="L10" pad="A"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="SCL1">
<contactref element="U1" pad="1"/>
<contactref element="PAD3" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="D9">
<contactref element="L27" pad="A"/>
<contactref element="L30" pad="A"/>
<contactref element="L33" pad="A"/>
<contactref element="L34" pad="C"/>
<contactref element="L35" pad="C"/>
<contactref element="L36" pad="C"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="D10">
<contactref element="L25" pad="A"/>
<contactref element="L28" pad="C"/>
<contactref element="L29" pad="C"/>
<contactref element="L30" pad="C"/>
<contactref element="L32" pad="A"/>
<contactref element="L35" pad="A"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="D11">
<contactref element="L26" pad="A"/>
<contactref element="L31" pad="C"/>
<contactref element="L29" pad="A"/>
<contactref element="L32" pad="C"/>
<contactref element="L33" pad="C"/>
<contactref element="L36" pad="A"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="GND3">
<contactref element="PAD5" pad="1"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="+5V3">
<contactref element="PAD6" pad="1"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="SDA3">
<contactref element="U3" pad="5"/>
<contactref element="PAD8" pad="1"/>
</signal>
<signal name="D12">
<contactref element="L25" pad="C"/>
<contactref element="L28" pad="A"/>
<contactref element="L26" pad="C"/>
<contactref element="L31" pad="A"/>
<contactref element="L27" pad="C"/>
<contactref element="L34" pad="A"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="SCL3">
<contactref element="U3" pad="1"/>
<contactref element="PAD7" pad="1"/>
</signal>
<signal name="N$3">
</signal>
<signal name="D17">
<contactref element="L51" pad="A"/>
<contactref element="L54" pad="A"/>
<contactref element="L57" pad="A"/>
<contactref element="L58" pad="C"/>
<contactref element="L59" pad="C"/>
<contactref element="L60" pad="C"/>
<contactref element="U5" pad="7"/>
</signal>
<signal name="D18">
<contactref element="L49" pad="A"/>
<contactref element="L52" pad="C"/>
<contactref element="L53" pad="C"/>
<contactref element="L54" pad="C"/>
<contactref element="L56" pad="A"/>
<contactref element="L59" pad="A"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="D19">
<contactref element="L50" pad="A"/>
<contactref element="L55" pad="C"/>
<contactref element="L53" pad="A"/>
<contactref element="L56" pad="C"/>
<contactref element="L57" pad="C"/>
<contactref element="L60" pad="A"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="GND5">
<contactref element="PAD17" pad="1"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="+5V5">
<contactref element="PAD18" pad="1"/>
<contactref element="U5" pad="8"/>
</signal>
<signal name="SDA5">
<contactref element="U5" pad="5"/>
<contactref element="PAD20" pad="1"/>
</signal>
<signal name="D20">
<contactref element="L49" pad="C"/>
<contactref element="L52" pad="A"/>
<contactref element="L50" pad="C"/>
<contactref element="L55" pad="A"/>
<contactref element="L51" pad="C"/>
<contactref element="L58" pad="A"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="SCL5">
<contactref element="U5" pad="1"/>
<contactref element="PAD19" pad="1"/>
</signal>
<signal name="N$4">
</signal>
<signal name="D21">
<contactref element="L63" pad="A"/>
<contactref element="L66" pad="A"/>
<contactref element="L69" pad="A"/>
<contactref element="L70" pad="C"/>
<contactref element="L71" pad="C"/>
<contactref element="L72" pad="C"/>
<contactref element="U7" pad="7"/>
</signal>
<signal name="D22">
<contactref element="L61" pad="A"/>
<contactref element="L64" pad="C"/>
<contactref element="L65" pad="C"/>
<contactref element="L66" pad="C"/>
<contactref element="L68" pad="A"/>
<contactref element="L71" pad="A"/>
<contactref element="U7" pad="2"/>
</signal>
<signal name="D23">
<contactref element="L62" pad="A"/>
<contactref element="L67" pad="C"/>
<contactref element="L65" pad="A"/>
<contactref element="L68" pad="C"/>
<contactref element="L69" pad="C"/>
<contactref element="L72" pad="A"/>
<contactref element="U7" pad="3"/>
</signal>
<signal name="GND6">
<contactref element="PAD25" pad="1"/>
<contactref element="U7" pad="4"/>
</signal>
<signal name="+5V6">
<contactref element="PAD26" pad="1"/>
<contactref element="U7" pad="8"/>
</signal>
<signal name="SDA7">
<contactref element="U7" pad="5"/>
<contactref element="PAD28" pad="1"/>
</signal>
<signal name="D24">
<contactref element="L61" pad="C"/>
<contactref element="L64" pad="A"/>
<contactref element="L62" pad="C"/>
<contactref element="L67" pad="A"/>
<contactref element="L63" pad="C"/>
<contactref element="L70" pad="A"/>
<contactref element="U7" pad="6"/>
</signal>
<signal name="SCL7">
<contactref element="U7" pad="1"/>
<contactref element="PAD27" pad="1"/>
</signal>
<signal name="N$7">
</signal>
<signal name="D25">
<contactref element="L75" pad="A"/>
<contactref element="L78" pad="A"/>
<contactref element="L81" pad="A"/>
<contactref element="L82" pad="C"/>
<contactref element="L83" pad="C"/>
<contactref element="L84" pad="C"/>
<contactref element="U8" pad="7"/>
</signal>
<signal name="D26">
<contactref element="L73" pad="A"/>
<contactref element="L76" pad="C"/>
<contactref element="L77" pad="C"/>
<contactref element="L78" pad="C"/>
<contactref element="L80" pad="A"/>
<contactref element="L83" pad="A"/>
<contactref element="U8" pad="2"/>
</signal>
<signal name="D27">
<contactref element="L74" pad="A"/>
<contactref element="L79" pad="C"/>
<contactref element="L77" pad="A"/>
<contactref element="L80" pad="C"/>
<contactref element="L81" pad="C"/>
<contactref element="L84" pad="A"/>
<contactref element="U8" pad="3"/>
</signal>
<signal name="GND7">
<contactref element="PAD29" pad="1"/>
<contactref element="U8" pad="4"/>
</signal>
<signal name="+5V8">
<contactref element="PAD30" pad="1"/>
<contactref element="U8" pad="8"/>
</signal>
<signal name="SDA8">
<contactref element="U8" pad="5"/>
<contactref element="PAD32" pad="1"/>
</signal>
<signal name="D28">
<contactref element="L73" pad="C"/>
<contactref element="L76" pad="A"/>
<contactref element="L74" pad="C"/>
<contactref element="L79" pad="A"/>
<contactref element="L75" pad="C"/>
<contactref element="L82" pad="A"/>
<contactref element="U8" pad="6"/>
</signal>
<signal name="SCL8">
<contactref element="U8" pad="1"/>
<contactref element="PAD31" pad="1"/>
</signal>
<signal name="N$8">
</signal>
<signal name="D29">
<contactref element="L87" pad="A"/>
<contactref element="L90" pad="A"/>
<contactref element="L93" pad="A"/>
<contactref element="L94" pad="C"/>
<contactref element="L95" pad="C"/>
<contactref element="L96" pad="C"/>
<contactref element="U9" pad="7"/>
</signal>
<signal name="D30">
<contactref element="L85" pad="A"/>
<contactref element="L88" pad="C"/>
<contactref element="L89" pad="C"/>
<contactref element="L90" pad="C"/>
<contactref element="L92" pad="A"/>
<contactref element="L95" pad="A"/>
<contactref element="U9" pad="2"/>
</signal>
<signal name="D31">
<contactref element="L86" pad="A"/>
<contactref element="L91" pad="C"/>
<contactref element="L89" pad="A"/>
<contactref element="L92" pad="C"/>
<contactref element="L93" pad="C"/>
<contactref element="L96" pad="A"/>
<contactref element="U9" pad="3"/>
</signal>
<signal name="GND8">
<contactref element="PAD33" pad="1"/>
<contactref element="U9" pad="4"/>
</signal>
<signal name="+5V9">
<contactref element="PAD34" pad="1"/>
<contactref element="U9" pad="8"/>
</signal>
<signal name="SDA9">
<contactref element="U9" pad="5"/>
<contactref element="PAD36" pad="1"/>
</signal>
<signal name="D32">
<contactref element="L85" pad="C"/>
<contactref element="L88" pad="A"/>
<contactref element="L86" pad="C"/>
<contactref element="L91" pad="A"/>
<contactref element="L87" pad="C"/>
<contactref element="L94" pad="A"/>
<contactref element="U9" pad="6"/>
</signal>
<signal name="SCL9">
<contactref element="U9" pad="1"/>
<contactref element="PAD35" pad="1"/>
</signal>
<signal name="N$9">
</signal>
</signals>
</board>
</drawing>
</eagle>
